KNX SO250 tank sensor invitation to tender

Tank sensor for the KNX bus system for recording the liquid level in tanks and for distance measurement Consisting of an evaluation unit and an ultrasonic measuring sensor. Evaluation unit with display and keypad (level/distance display, measurement setting). Interfaces: KNX bus plug-in terminal, 2 additional output relays. Auxiliary voltage 230 V. Configuration via ETS: 5 threshold values, 57 communication objects.
Media-resistant measuring sensor for water and heating oil, measuring range 12…250 cm.
Dimensions: Evaluation unit for rail mounting (7 width units), 123 x 89 x 61 (W x H x D in mm). Sensor diameter approx. 60 mm, height approx. 45 mm, thread 1½ inches, cable length 10 m.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70151 KNX SO250

KNX SO250 basic tank sensor invitation to tender

Tank sensor for the KNX bus system for recording the liquid level in tanks and for distance measurement Consisting of evaluation unit and ultrasonic measuring sensor, connection via BNC plug. Bus communication and power supply via KNX bus plug-in terminal. Configuration via ETS: 5 threshold values, 57 communication objects.
Media-resistant measuring sensor for water and heating oil, measuring range 12…250 cm.
Dimensions: Evaluation unit for rail mounting (3 width units), 53 x 88 x 60 (W x H x D in mm). Sensor diameter approx. 60 mm, height approx. 45 mm, thread 1½ inches, cable length 10 m.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70153 KNX SO250 basic