Suntracer KNX sl light weather station invitation to tender

Weather station for the KNX bus system. Recording of brightness, wind speed, precipitation (heated sensor), temperature. Calculation of the sun's position. GPS receiver (time, date, position), calendar and week timer. Integrated shading control, shadow edge and lamella tracking for 5 façades. Frost protection for shading elements. Summer compensation for cooling systems. 8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, survey of conditions, transition. 864 communication objects. 
Integrated mount for wall/mast mounting.
Dimensions 62 x 71 x 145 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70155 Suntracer KNX sl light